Scale USB Interface

Install **UsbHidApi USB Comm Library** by unzipping and running the installer from Kadtronix. It can be downloaded from <http://www.kadtronix.com/downloads/usbhidapi11Csetup.zip>

The setup installs drivers and demo application in “C:\Program Files\USB HID Demo” folder. You can run the application and it will show “Metler” as one of the devices installed. I rebooted the PC after installation without trying to run the app, so I did not test if the reboot is necessary. After the reboot Demo application worked and displayed the device and the model number.

I experienced problems reading the scale from CashierLive until I disabled PosCom.ocx in IE via “Manage Add-ons” and deleted it from “C:\Windows\Downloaded Program Files”. After reinstalling POS control, scale worked.